{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Parameter-Liste Hyperion 3D DE","Parameter List Hyperion 3D EN"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Parameter-Liste Hyperion 3D DE","index":0,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":false,"merged":[[2,1,2,2],[3,1,3,2],[5,1,5,2],[26,0,26,2]]}
["Hyperion 3D Parameter-Liste "]
[]
["Installationsstandort:"]
[]
["Installiert durch:"]
["Datum:"]
[]
["Parameter","Haupt-Sensor","Neben-Sensor"]
["Position vom Sensor","innen / aussen","innen / aussen"]
[]
["Detektionsbereich Breite","m","m"]
["Detektionsbereich Tiefe","m","m"]
[]
["Vorfeld Breite","m","m"]
["Vorfeld Tiefe","m","m"]
[]
["Sicherheitsabstand","m"]
["Schliessverzögerung","sek"]
["Objektunterdrückung","Keine / Personen","Keine / Personen"]
["Querverkehrsoptimierung","Ja / Nein","Ja / Nein"]
["Höhensensor","Ja / Nein"]
["Manuelle Schliesszeit","sek"]
["Virtueller Öffnungstaster","Ja / Nein","Ja / Nein"]
["Objekthöhe für Vollöffnung","m"]
["Minimale Öffnungshöhe","m"]
["Sleep Mode","Ja / Nein","Ja / Nein"]
["Achtung: Ist der Parameter \"Sleep Mode\" aktiv, müssen 5-48 VDC am Digitaleingang anstehen, damit der Sensor in Betrieb geht."]

{"sheet":"Parameter List Hyperion 3D EN","index":1,"n_rows":27,"n_cols":3,"rows_kept":27,"cut":false,"hidden":false,"merged":[[2,1,2,2],[3,1,3,2],[4,1,4,2],[5,1,5,2],[26,0,26,2]]}
["Hyperion 3D Parameter List "]
[]
["Place of installation:"]
[]
["Installed by:"]
["Date:"]
[]
["Parameter","Master sensor","Slave sensor"]
["Position of sensor","inside / outside","inside / outside"]
[]
["Detection zone width","m","m"]
["Detection zone depth","m","m"]
[]
["Presence zone width","m","m"]
["Presence zone depth","m","m"]
[]
["Safety distance","m"]
["Closing delay","sec"]
["People / vehicle separation","None / People","None / People"]
["Cross traffic optimisation","Yes / No","Yes / No"]
["Height sensor installed","Yes / No"]
["Manual closing timeout","sec"]
["Virtual open button","Yes / No","Yes / No"]
["Object height for full opening","m"]
["Minimum opening height","m"]
["Sleep mode","Yes / No","Yes / No"]
["Remark: When the paramter \"sleep mode\" is active, sensor requires 5-48VDC on digital input to operate."]